April 2002

The steps detailed below describe the recommended procedure to install printer drivers on a Citrix MetaFrame and Windows NT4 Terminal Services.  

For information on installing drivers for Novell Point and Print or NDPS environments, please refer to following document Novell NDPS and Point and Print Installation.

Citrix Metaframe and Windows NT4 Terminal Services 

When installing a printer onto a Windows NT4 Server with Terminal Services along with Citrix Metaframe, for optimum performance Kyocera recommends using the Kyocera Minidriver.  This driver is located in the following location:

•	Drivers/Other/PCL/NT4/1Gpd_based/English 

Kyocera also recommends using the Microsoft “Add Printer Wizard” to install the printer.
Follow the steps listed below to install the printer using the Kyocera Minidrivers.

1.	Click on the windows “Start” button, scroll up and highlight “Settings”.
2.	Highlight and click on “Printers”.

3.	This will invoke the “Printers” dialog box.  Double click on the “Add Printer” icon.
4.	The “Add Printer Wizard” screen will now appear.

5.	Select the “My Computer” radio button, then select “Next”.

6.	Next select the port location of the printer: “LPT1”, then select “Next”.

7.	The Next screen is for the Printer Driver Selection. Select the “Have Disk” button.

8.	The next screen to be invoked will be requesting the location of the Driver files. Select the “Browse” button.

9. Next select the Letter that corresponds to the Letter of your CD-Rom drive.

      10.  Select the “Drivers” folder.

11.	Select the “Other”folder.

12.  Next select the “PCL” folder.

13.  Next select the “NT4” folder.

14.	 Next select the “1Gpd_based” folder.

  15.  Double Click on the “English”  folder.

16.   Last select “Open”, then select “OK”

17.	Now you may select your Printer Model from the Printer selection box and then select “Next”.

18.  You may name your Printer or keep the default name and then select “Next”.

19.	Select the “Shared’ radio button to allow other users to access your Printer.
Enter the “Share Name” in the edit box

    

20.	Select all additional Operating Systems that will have access to the Shared     
      Printer.

21.	Select the “Yes” radio button and then select the “Finish” button to print a test page and verify proper Printer Installation.

22.	Now you will see the newly created Printer Icon appearing in the Printers folder.
You are now ready to print and have completed the installation.

April 2002

The drivers in this directory are for use with Novell NDPS and Point and Print (queue based non-NDPS) printing.  This guide will show you how to install these drivers for use in these Novell printing methods.
Novell NDPS and Point and Print Installation

NDPS or Novell Distributed Print Services gives an administrator centralized control and status monitoring of printers anywhere on the network.  It allows the administrator to upload drivers to one centralized place using a broker.  Users can then connect to the printer and the drivers download automatically.  NDPS first appeared in Netware 5.  For more information on NDPS click here.

Point and Print is another way of setting up printers in a Novell environment.  Drivers are assigned to a non-NDPS print queue and loaded to a holding place.  When a user connects to the printer, the driver downloads from the holding place and installs the printer on the user’s machine.  

The drivers you need to use for Novell are located in the following directories:

For NDPS:
\\drivers\Novell\NDPS\NT4_Win2K
\\drivers\Novell\NDPS\Win9x_ME

For Point and Print:
\\drivers\Novell\Point and Print\NT4_Win2K
\\drivers\Novell\Point and Print\Win9x_ME 

NDPS
Use the following steps to load the drivers to the broker.  Make sure the drivers are not set to read only.  You may have to copy the drivers to the local machine, select the files and uncheck the read only box.  This is a known issue within the Novell and is to be fixed in a subsequent release.

1.	Open NWAdmin 
2.	Double click on the Broker which you are loading drivers to
3.	Click on Resource Management (RMS)
4.	Click Add resources
5.	Choose the OS for the drivers you wish to upload
6.	Click Add
7.	Click Browse
8.	Select the .inf file of the printer model you wish to load.
9.	In a few moments the driver will be loaded into the RMS.

Drivers get loaded to this location:
\\{server name}\SYS\ndps\resdir\{LANGUAGE}\prndrv\{driver os}
Example:  \\NW51\SYS\ndps\resdir\ENGLISH\prndrv\windows 2000

Point & Print
You will need MSPRINT.INF, MSPRINT2.INF and LAYOUT.INF for uploading Win9x drivers from NT (located in precopy2.cab on the Win98 CD).  You will need NTPRINT.INF from the I386 folder on the NT/2000 CD to load these drivers from Win9X.  They are not required if you load the drivers from it’s partner OS (ie load the Win9x drivers from Win98 and load the NT drivers from NT).

The default repository for the Point and Print drivers is
\\{server name}\SYS\ LOGIN\{OS}\print\drivers\{language code number}
For example \\NW51\SYSLOGIN\w2kx86\print\drivers\9

In Windows NT and Windows 2000:
1.	Open My Network Places/Network Neighborhood 
2.	Click on Novell Connections 
3.	Browse thru the context (start from the Tree) to the printer queue.  
4.	Right click on the queue
5.	Click Properties 
6.	On the Properties page in the NetWare Queue tab, the Type must show as Novell Directory Services Queue.
7.	On the Setup Point and Print tab choose the OS of the driver you want to upload.
8.	Choose the language of the driver you wish to upload.
9.	Click Select Printer Model
10.	 Click Have Disk 
11.	 Browse to the path where the drivers are located.
12.	 Select the driver you wish to upload and click Open.
13.	 It will then upload the drivers to its proper location.
14.	 On the Setup Point and Print tab – click Apply.

In Windows 9x:
1.	Open Network Neighborhood
2.	Browse thru the context (start from the Tree) to the printer queue.  
3.	Right click on the queue
4.	Click Properties 
5.	On the Properties page in the NetWare Queue tab, the Type must show as Novell Directory Services Queue.
6.	On the Setup Point and Print tab choose the OS of the driver you want to upload.
7.	Choose the language of the driver you wish to upload.
8.	Click Select Printer Model
9.	 Click Have Disk 
10.	 Browse to the path where the drivers are located.
11.	 Select the driver you wish to upload and click Open.
12.	 It will then upload the drivers to its proper location.
13.	 On the Setup Point and Print tab – click Apply.

Frequently Asked Questions

Q.	I can’t browse for drivers when I am trying to upload them to the broker.  How can I fix this?
A.	Right click on the shortcut to NWADMIN and go to properties.  Add the switch   “ / disabletlsmgr” (without quotes) to the Target Line.  For example: \\Nw60\SYS\PUBLIC\win32\nwadmn32.exe / disabletlsmgr 
 
Q.	In Windows 2000, when I am trying to upload drivers for a Point and Print setup for Windows 9x or NT I can not browse.
A.	This is a known issue.  You can browse and upload the drivers for Win2K, Win9x, and WinNT from both Win9x or WinNT.

Q.	I am trying to change drivers in NDPS, but the client won’t download the new driver.
A.	This is a known issue.  It is a problem with both automatic downloads and new installs.  In order for the drivers to download correctly, you need to do the following:
1.	Double click on the printer agent.
2.	Click Control.
3.	Click Set Defaults.
4.	Click on the Drivers tab.
5.	For each OS, under Available Drivers you should select [None] then click OK.
6.	Click Control.
7.	Click Set Defaults.
8.	Click on the Drivers tab.
9.	Then for each OS, select the driver you wish to use.
10.	Click OK

Q.	I can’t seem to be able to change the default directory that the Point and Print drivers get copied to.  How can I do that?
A.	There is a fix for this on Novell’s Support site.  The fix is described in TID #10024206.